
Multimeter Application
========================

The 'Multimeter' application is designed for simple fixed frequency analysis application.
It provides only a FixFs analysis channel with basic measurements (time domain values, spectrum, spectrogram).
There is no rotational speed input needed or provided.
The project has two vibration sensors, two virtual sensors for filtering and one "AnalogVal" control value (e.g. for measuring 
a simple voltage source, a position, whatever) as options. (De-)activate the according Tas box channels as needed.

The "Design Data" and kinematics model is empty: there is only the one 'NoiseSource' location needed for the FixFs resampling.

Modes and Measurements: There are two test steps, 'Runin' and 'NoiseTest'. The 'Runin' mode has no measurement values
except Rms-Min; all measurements are only defined for 'NoiseTest'. The 'Runin' mode is provided for use together with
the Automatic Test Sequence. (Obviously, the mode can be deleted or re-used for other purposes.)

Since there is no rotational speed, the project
assumes either external Measure On/Off commands or triggering by time. The following measurements are predefined:
RMS, Crest, Peak, Kurtosis and tracks of all these (using time as control value),
RMS Min
Spectrum and Spectrogram
Control Value Track for the (optional) 'AnalogVal' input.

The two virtual noise signals VSFilt are high pass filtered in the standard settings. If Microphones are used, A filter can be
activated. If no filtering is desired, it would make sense to delete the virtual signals from the database.
It is also advisable to delete the second vibration sensor if not used, thus also deleting all defined measured 
values, which would otherwise generate 'missing values' errors.

The project is prepared for UDP test stand communication. In addition, it contains the Automatic Serial Number plugin and
the Automatic Test Sequence plugin, but both are de-activated in the current settings.

