--------------------------------------------------------------------
TAS-Box 'A' (TAS 48) firmware versions:
--------------------------------------------------------------------
Box	Module	Element	Slot	Kind of MCU	Version	(Hex)	Date
A	Host interface	FX2LP	-	TAS48 FX2LP	10	0A	2019-03-14
A	USB	Control-MCU	-	USB	1	01	2019-07-15
A	USB	FPGA	-	-	2	02	2019-05-29
A	Power supply	Control-MCU	-	Pwr Supply	1	01	2019-07-15
A	Pulse	Control-MCU	0	TIS 26	1	01	2019-07-15
A	Pulse	FPGA	0	-	10	0A	-
A	ADC	Control-MCU	1	TAD48+ Ctrl	8	08	2019-01-16
A	ADC	Control-MCU	2	TAD48+ Ctrl	8	08	2019-01-16
A	ADC	Control-MCU	3	TAD48+ Ctrl	8	08	2019-01-16
A	ADC	Control-MCU	4	TAD48+ Ctrl	8	08	2019-01-16
--------------------------------------------------------------------
TAS-Box 'A' setup:
--------------------------------------------------------------------
A.0: TUI 07	Sampling frequency (block length): 50 kHz (82 ms)	
A.0: TIS 26	Active: False	Signal Source: <-1>	Puls Divider: 1	Led A: Off	Led B: Off	Edge Detect: Rising	Inhibit µs (+): 0	Inhibit µs (-): 0	Attenuation: False	High reference voltage: False	Mode: Transducer pulses	Input: (inactive)	
		Active: False	Signal Source: <-1>	Puls Divider: 1	Led A: Off	Led B: Off	Edge Detect: Rising	Inhibit µs (+): 0	Inhibit µs (-): 0	Attenuation: False	High reference voltage: False	Mode: Transducer pulses	Input: (inactive)	
		Active: False	Signal Source: <-1>	Puls Divider: 1	Led A: Off	Led B: Off	Edge Detect: Rising	Inhibit µs (+): 0	Inhibit µs (-): 0	Attenuation: False	High reference voltage: False	Mode: Transducer pulses	Input: (inactive)	
		Active: False	Signal Source: <-1>	Puls Divider: 1	Led A: Off	Led B: Off	Edge Detect: Rising	Inhibit µs (+): 0	Inhibit µs (-): 0	Attenuation: False	High reference voltage: False	Mode: Transducer pulses	Input: (inactive)	
A.1: TAD 48	Active: True	Signal Source: <11>	Input: Differential	Coupling: AC	Sensitivity: 1V	ICP operation: Standard	
		Active: True	Signal Source: <12>	Input: Differential	Coupling: AC	Sensitivity: 1V	ICP operation: Standard	
A.2: TAD 48	Active: False	Signal Source: <-1>	Input: Differential	Coupling: AC	Sensitivity: 1V	ICP operation: Standard	
		Active: False	Signal Source: <-1>	Input: Differential	Coupling: AC	Sensitivity: 1V	ICP operation: Standard	
A.3: TAD 48	Active: False	Signal Source: <-1>	Input: Differential	Coupling: AC	Sensitivity: 1V	ICP operation: Standard	
		Active: False	Signal Source: <-1>	Input: Differential	Coupling: AC	Sensitivity: 1V	ICP operation: Standard	
A.4: TAD 48	Active: False	Signal Source: <-1>	Input: Differential	Coupling: AC	Sensitivity: 1V	ICP operation: Standard	
		Active: False	Signal Source: <-1>	Input: Differential	Coupling: AC	Sensitivity: 1V	ICP operation: Standard	

--------------------------------------------------------------------
TasAlyser Version VC1929-64bit-Release-Build, Version 0.0.28.142 (Rev. 28142), Apr 25 2022
Project Number: (not set)

--------------------------------------------------------------------
Computer System Information:
--------------------------------------------------------------------
    MAC Addresses:
        00:BE:43:1B:C9:58  --> Intel(R) Ethernet Connection (13) I219-LM
        60:A5:E2:A1:FA:85  --> Bluetooth Device (Personal Area Network)
        00:09:0F:FE:00:01  --> Fortinet Virtual Ethernet Adapter (NDIS 6.30)
        00:09:0F:AA:00:01  --> Fortinet SSL VPN Virtual Ethernet Adapter
        00:BE:43:1B:C9:59  --> Realtek USB GbE Family Controller #2
        60:A5:E2:A1:FA:81  --> Intel(R) Wi-Fi 6 AX201 160MHz
        60:A5:E2:A1:FA:82  --> Microsoft Wi-Fi Direct Virtual Adapter
        62:A5:E2:A1:FA:81  --> Microsoft Wi-Fi Direct Virtual Adapter #2
--------------------------------------------------------------------
